How to Install KemNet (Ver 5.0)

NOTE: There are two versions of KemNet.   The legacy version 4.21 is for use with controllers that have serial numbers of
56016 and lower.   This new version 5.0 is for use with temperature and vacuum controllers that have serial number of 
56017 and higher.

Download KemNet 5.0.zip from the J-KEM website.
Unzip the file.
Open the resulting folder titled KEM-Net 5.0.
Open the folder titled KEM-Net Application.
A copy of the KEM-Net User Manual is also in this folder.
Double click on the file Setup.exe, then accept all of the default settings during installation.
The drivers for KEM-Net are native to all versions of Windows 10 and 11, so separate installation of the drivers should not 
be required.   But, if needed, copies of the drivers are located in the folder titled Other Items.

Other Items
In the Other Items folder is contained a copy of the KEM-Net drivers if needed.
For users who would like to write their own application to communicate with J-KEM's controllers, helpful information can 
be found in the folder titled Automation Assistance.   For advanced programmers, the full Modbus protocol for communicating
with the J-KEM 3300 meter is available on request.


